**Optimization of open-cell foam catalyst macrostructure for mutual detoxication of NO and CO**

**Mitrichev Ivan Igorevich**, D. Mendeleev University of Chemical Technology of Russia, PhD student, lead programmer Computer Information Technologies chair, 9, Miusskaya sq., Moscow, 125047, Russia, fax +74956092964, phone + 74954952126, imitrichev@muctr.ru

**Vardanyan Andranik Eduardovich**, D. Mendeleev University of Chemical Technology of Russia, 4th year student, Computer Information Technologies chair, 9, Miusskaya sq., Moscow, 125047, Russia, fax +74956092964, phone + 74954952126, kolts@muctr.ru

**Jhensa Andrey Vyacheslavovich**, D. Mendeleev University of Chemical Technology of Russia, PhD, assistant professor, Computer Information Technologies chair, 9, Miusskaya sq., Moscow, 125047, Russia, fax +74956092964, phone + 74954952126, kolts@muctr.ru

**Koltsova Eleonora Moiseevna**, D. Mendeleev University of Chemical Technology of Russia, Doctor of Technical Sciences, professor, head of Computer Information Technologies chair, 9, Miusskaya sq., Moscow, 125047, Russia, fax +74956092964, phone + 74954952126, kolts@muctr.ru

***Keywords****: open-cell foam, catalyst, optimization, mathematical modelling, nitrogen oxide, carbon monooxide, waste gas purification.*

Waste gas purification from NO and CO is an important problem for environmental catalysis. The influence of state-of-the-art highly porous foam catalyst macrostructure on conversion in the process concerned is studied by means of mathematical modeling and computer simulation. The degree of mutual neutralization of NO and CO is mainly dependent on the total catalyst area. At equal active component loading and equal surface area the foam with the highest porosity possesses the lowest pressure drop. Foam with a lower porosity gives insignificantly higher conversion in conjunction with a strong increase in pressure drop. A material with a high number of pores per inch should be used to reduce the catalyst length that is required for the prescribed conversion value.

**References**

1. Grunskiy V.N. Low-volume cellular structured catalytic systems with high adjustable outer surface area. Doctor thesis. M., 2009. (in Russ.).

2. Antsiferov V.N., Makarov A.M., Ostroushko A.A. Powder Materials Problems. Ch. VII: Highly porous cellular materials – prospective catalyst support. Yekaterinburg: UrO RAN, 2006. 228 p. (in Russ.).

3. Garbaruk A.V. Viscous fluid flow and turbulence models: Methods for calculating turbulent flows: lecture notes. SPb.: Sankt-Peterburgskiy gosudarstvennyy politekhnicheskiy universitet, 2010. 127 p. (in Russ.).

4. Mitrichev I.I., Koltsova E.M., Zhensa A.V. Computer simulation of gasodynamic conditions in channels of open-cell foam. Fundamental'nye issledovaniya [Fundamental Research], 2012, no. 11(2). pp. 440-446 (in Russ.).

5. Boomsma K., Poulikakos D. The effects of compression and pore size variations on the liquid flow characteristics in metal foams. Journal of fluids engineering, 2002, no. 124(1), pp. 263-272.

6. Milligan B., Ray S. F. Recent improvements in the measurement and control of ceramic foam filter quality. Proc. Int. Conf. Advances in Production and Processing of Aluminum, Manama, Bahrain, 2001. 15 p.

7. Lisova N.S., Mitrichev I.I., Koltsova E.M. Determination of kinetic parameters of NO+CO reaction. Uspekhi v khimii i himicheskoy tekhnologii [Advances in Chemistry and Chemical Technology], 2015, no. 163, pp. 60-62 (in Russ.).

**A method of separating para-nitrotoluene from a mixture of isomers of mononitrotoluene**

**Solovyov Sergey Aleksandrovich**, engineer-technologist Federal State Enterprise «Biysk Oleum Plant»; e-mail: briz@boz.biysk.ru

**Zvezdkin Vladimir Mikhailovich,** Deputy Chief of the science and technology center, Federal State Enterprise «Biysk Oleum Plant»; e-mail: briz@boz.biysk.ru

***Keywords****: para-nitrotoluene, sulfuric acid, freezing, mononitrotoluene, dinitrotoluene, isopropyl alcohol, sulfite-soda solution, crystallization, carbamide.*

The scope of Para–nitro toluene are described and point need for different industrial branches. Advantages and disadvantages of three basic ways of production of Para–nitro toluene analyzed.

The evidence shows that release in the company is economically feasible, where get trinitrotoluene and sulfuric acid. Described the methods of allocation Para–nitro toluene by method of freezing in the medium of sulfuric acid and its purification with isopropyl alcohol and sulfite soda solution at laboratory and experienced setting, and also construction of the main equipment.

It is showed method of allocation of Para–nitro toluene with using sulfuric acid allow get a ready–made products with high quality and output. It is considered a method of regeneration of isopropyl alcohol.

**References**

1. Berkman B.E. Indastrial synthesis of aromatic nitro compounds and amines.//M.: Chemistry, 1964.( in Russ ).
2. Kachaev V.A., Zenkov V.F., Valechnij S.I., Il'in V.P. RF № 2323205. A method for isolating 4-nitrotoluene. RU № 2323205. 2008. ( in Russ ).
3. Zbarskij V.L., Zhilin V.F. Toluene end nitro derivatives. // M.: Chemistry, 2000. (in Russ ).

 4. Vlasov O.M., Plyaskin O.YU., Solovjov S.A., Kadulin V.V., Zhamilova Z.A. Amethod for isolating 4-nitrotoluene.. RU № 2560882. 2015. ( in Russ ).

 The patentee: Federal State Compane «Biysk Oleum Factory».

5. References sulfuric acid worker. M.: Chemistry, 1971. ( in Russ ).

 6. The chemistry of the nitro and nitroso groups/ Edited H. Foeuer.–M.: World, 1973. ( in Russ ).

**Low-waste technology for production of 2',4,4'-trinitrobenzanilide, preproduct of 5(6)-amino-2-(4-aminophenyl)benzimidazole**

**Nadezhda V. Zavyalova**

Limited Liabiliy Company “Phenyl” (LLC «Phenyl»), Tula. research engineer.

e-mail: nadina86@rambler.ru

e-mail: vifed45@mail.ru

**Yevgeny L. Vulakh**

Limited Liabiliy Company “Phenyl” (LLC «Phenyl»), Director General, Doctor of Chemistry, Professor.

Address: 300026, Tula, Skuratovskaja St., 98.

e-mail: vulphenyl@mail.ru

***Keywords****:**2´,4,4´-trinitrobenzanilide, 5(6)-amino-2-(4-aminophenyl)-benzimidazole,**acylation,**kinetics.*

Synthesis of 2',4,4'-trinitrobenzanilide by aclation of 2,4-dinitroaniline by 4-nitrobenzoilchloride, catalized by ferric chloride (III), is performed in chlorbenzene media. Recycle of chlorbenzene mother liquid after separation of 2',4,4'-trinitrobenzanilide guarantees simplification of the process, increase of output and significant decrease in the amount of waste. Aclation of 2,4-dinitroaniline is inhibited both by the main product and by reaction of by-product, 4-nitrobenzoic acid anhydride, which forms complexes with the catalyst. Formation mechanisms for 4-nitrobenzoic acid anhydride, effect of 4-nitrobenzoic acid and it is anhydride on the rate of acylation reaction of 2,4-dinitroaniline nibu 4-nitrobenzoilchloride in chlorbenzene in the presence of ferric chloride (III), synthesis mechanisms for 2',4,4'-trinitrobenzanilide with implementation of chlorbenzene mother liquid have been investigated. Samples of 5(6)-amino-2-(4-aminophenyl)benzimidazole have been synthesized and characterized.

**References**

Chernyih T.E., Shorin S.V., Kuyantseva I.F. and etc. The molded item. RU N2017866. IPC D01F6/80., 1994 (in Russ.).

Chernyih T.E., Shorin S.V., Shiyanova L.B. and etc.Method of obtaining aromatic copolyamides (options) and creating high-tenacity high-modulus threads on their basis.., RU N2469052. IPC C08G69/32, D01F6/80 N34, 2012 (in Russ.).

Shuang Wang, Hongwei Zhou, Guodong Dang. Synthesis and Characterization of Thermally Stuble, High-Modulus Polyimides Containing Benzimidazole Moeieties. // J. Polymer Science: Part A: Polymer Chemistry. 2009. Vol. 47, pp. 2024–2031.

Morozova V.Ya., Brandina L.M.. Novokhatka D.A., Vulakh E.L. Technology for production of 2',4,4'-trinitrobenzanilide – preproduct of 5(6)-amino-2-(4-aminophenyl)benzimidazole synthesis. // Proizvodnyie benzimidazola i drugih aromaticheskih sistem v sinteze monomerov: mezhvuz. sb. nauch. tr. [Derivatives of benzimidazole and other aromatic systems in the synthesis of monomers: interuniversity. col. of scientific works] / Leningrad: LTI named after Lensovet. – 1982. – pp. 23–33 (in Russ.).

Chernobrovkina M.N., Vulakh E.L., Ivanova V.M. and etc. Mechanisms for anhydride production by interaction of aromatic carboxylic acids with acid chlorides. // Osnovnoy organicheskiy sintez i neftehimiya: sb. nauch. tr. [Heavy organic synthesis and petrochemistry: col. of scientific works] / Yaroslavl Polytechnic Institute. – Yaroslavl, 1989. – Issue 25. – pp. 90–98 (in Russ.).

Gutman V. Coordination chemistry in non-aqueous solutions. // M.: World, 1971.

Friedel-Crafts and Related Reaction. / Ed. G.A. Olah. New York; London: Intersci. Publ., 1963. – Vol. 1. – pp. 367–397.

Satchell D.P.N., Wardell J.L. Equilibria between stannic chloride and carboxylic acids in o-dichlorobenzene. // Trans. Faraday Soc., 1965. – Vol. 61. – no. 510. – Pt. 6. – pp. 1132–1137.

Myakisheva E.A., Kaminskiy A.Ya., Chinenova A.V. Finding 2,4-dinitroaniline and 2',4,4'-trinitrobenzanilide in case of their combined occurrence. // Metody analiza i kontrolya kachestva produktsii: nauch.-tehnich. referativnyiy sb. [Methods of analysis and quality control of outputs: scientific and technical reference col.] / NIITEHIM. – M. – 1982. – pp. 33–35 (in Russ.).

Shmid R., Sapunov V.N. Informal kinetics. Finding ways of chemical reactions. Translated from English. // M.: World, 1985 (in Russ.).

Chichibabin A.E. Basic principles of organic chemistry. // M.: Goshimizdat, 1954. – Vol. 1 (in Russ.).

General workshop on organic chemistry. Translated from German ed. A.N. Kost. // M.: World, 1965 (in Russ.).

 Laidler K. Kinetics of organic reactions. Translated from English ed. I.P. Beletskaya, N.F. Kazanskaya. // M.: World, 1966 (in Russ.).

Ashmor P.A. Catalysis and inhibition of chemical reactions. // M.: World, 1966 (in Russ.).

 Vulakh E.L., Morozova V.Ya., Nemleva S.A. and etc. Competitive inhibition in the acylation reaction of 2,4-dinitroaniline with 4-nitrobenzoylchloride in the presence of ferric chloride. // Sintez i tehnologiya monomerov: sb. nauch. tr. [Synthesis and technology of monomers: col. of scientific works] / VNIPIM. – M.: NIITEHIM. – 1987. – pp. 78–83 (in Russ.).

**Regularities of macroscopic kinetics of the isobutylene with isoprene copolymerization under conditions of intense turbulent fluctuations**

**Tereshchenko Konstantin Alekseevich**

«Kazan National Research Technological University», Associate Professor of Department of Processing Technology of Polymers and Composite Materials,

Address:420015, Kazan, Karl Marks st. 68

Phone No 8(843)231-95-46

e-mail:nucleurmind@yandex.ru

**Ulitin Nikolai Victorovich**

«Kazan National Research Technological University»**,** Professor of Department of Processing Technology of Polymers and Composite Materials,

Address:420015, Kazan, Karl Marks st. 68

Phone No 8(843)231-95-46

e-mail:n.v.ulitin@mail.ru

***Keywords:*** *butyl rubber, isobutylene, isoprene, suspension copolymerization, physical and chemical hydrodynamics.*

It is for the first time that physical and chemical hydrodynamics of cationic suspension copolymerization process of isobutylene with isoprene was studied by the method of numerical experiment (the catalyst is AlCl3, the solvent is CH3Cl, temperature ≥ 173 K; the reaction volume was limited by a cylinder, where intense turbulent fluctuations were created) It has been established that with the decrease of size of the reaction zone (cylinder diameter from 0.2 to 0.1 m.) and speed of the reaction slurry (from 10 to 1 m. / s.) the decrease is happening of the number average (from 91 700 to 1360) and weight average (from 257 000 to 134 000) molecular weight of the synthesized butyl, and an increase of its polydispersity is taking place (from 2.8 to 110).

**References**

1. Ulitin N.V., Tereshchenko K.А. Physical and chemical hydrodynamics of cationic copolymerization of isobutylene with isoprene. Khimicheskaya promyshlennost' segodnya [Chemical industry today], 2015, no., pp. (in Russ.).

2. Ulitin N.V., Tereshchenko K.А. Model of chemical kinetics and identification of cationic copolymerization of isobutylene with isoprene kinetic constants. Khimicheskaya promyshlennost' segodnya [Chemical industry today], 2015, no., pp. (in Russ.).

3. Deberdeev R.Ya., Berlin A.A., Dyakonov G.S., Zakharov V.P., Monakov Yu.B. Fast chemical reaction in turbulent flows: theory and practice. Shawbury: Smithers Rapra Technology Ltd, 2013.

4. Sangalov Yu.A., Minsker K.S., Zaikov G.E. Polymers derived from isobutylene. Synthesis, properties, application. Utrecht: VSP, 2001.

5. Butyl Rubber: A techno-commercial profile. Chemical Weekly, 2009, V. 55, no. 12, pp. 207-211.

**The comparative analysis of methods helium extraction from natural gas and fields their effective application.**

**Troinikov Anton Dmitrievich**

D. Mendeleyev University of Chemical Technology of Russia, postgraduate student, chair of membrane technology.

Address: Miusskaya sq., 9, 125047 Moscow, Russia

e-mail: antontroynikov@mail.ru

PJSC «VNIPIgazdobycha», engineer of the 1st category, prospective development division.

Address: 4 Sacco & Vanzetti St., Saratov, 410012, Russian Federation.

**Kagramanov Georgy Gajkovich**

D. Mendeleyev University of Chemical Technology of Russia, Doctor of Technical Sciences, Professor, Head of chair of membrane technology.

Address: Miusskaya sq., 9, 125047 Moscow, Russia

e-mail: kagri@muctr.ru

**Kislenko Nataliya Nikolaevna**

PJSC «VNIPIgazdobycha», PhD in Technical Sciences, Corresponding Member of the Russian Academy of Natural Sciences, Deputy Head of Pre-project engineering Department.

Address: 4 Sacco & Vanzetti St., Saratov, 410012, Russian Federation.

***Keywords:*** *helium, helium extraction, Eastern Siberia, membrane technology, membrane separation, cryogenic technology, adsorption, helium storage.*

Different hinds of technologies, ensuring helium extraction from the helium-rich natural gas are given. It is shown that the use of cryogenic helium allocation method is the most effective in the production of LNG, to produce helium and hydrocarbon fractions, as well as in cases of removal of nitrogen from helium-rich gas with the simultaneous production of hydrocarbon fractions. Absorption method is useful when the production of marketable helium from concentrate helium in which helium content exceeds 50 vol. %. Membrane separation technology helium is most effective for problems of excess allocation against market requirements quantities of helium, with a view to their destinations on long-term storage in isolated deposits of the producing fields.

**References**

1. Mkrtychyan Ya. S., Lugaj D.V., Ruban G.N. et al. Helium in Russia. Helium and its role in addressing key issues of scientific and technological progress Book 1. // Moscow, Neftegaz, 2012, 215 р. (in Russ.).
2. Panteleev D.V., Stolypin E.V., Volchenko A.G., Syrkin A.M. Development of helium industrial production in Gazprom dobycha Orenburg, LLC // Neftegazovoe delo, [Oil and Gas Business], 2011, №2, pp. 128-135 (in Russ.).
3. Ogrel L.D. Prospects for Russia in the helium market. // Gazovaja promyshlennost' [Gas Industry] №701, 2014, pp. 22-23 (in Russ.)..
4. Yakutseni V.P. Helium resource base in the world and the prospects of helium industry development // Neftegazovaya Geologiya. Teoriya I Praktika. 2009, V.4, №2 (in Russ.). URL: http://www.ngtp.ru/rub/3/15\_2009.pdf
5. Saeid Mokhatab, William A. Poe, John Y. Mak. Handbook of Natural Gas Transmission and Processing, 3rd Edition Principles and Practices // Amsterdam, Gulf Professional Publishing is an imprint of Elsevier, 2015. p. 628.
6. Conrado Rillo Millán, Leticia Tocado Martínez. U.S. Patent 8973397, 2015.
7. Murin V.V., Kislenko N.N. et al. Technology for processing natural gas and condensate: Hand-Book: 2 vols. // Moscow, Nedra, 2002, vol. 1, p. 517 (in Russ.).
8. Molchanov S.A., Samakaeva T.O. Complex training and processing of multi-component natural gases in the a gas chemical complexes. // Moscow, Nedra, 2013, p. 514 (in Russ.).
9. Lapidus A.L., Golubeva I.A., Zhagfarov F.G. Gas Chemistry. // Moscow, CentrLitNefteGaz, 2008. p. 447. (in Russ.).
10. Campbell J.M. Gas Conditioning and Processing, v.2 The Equipment Modules. 7th edition. // Campbell Petroleum Series, 1992, p. 444.
11. Han S.A., Igoshin A.I., Kazarjan V.A., Skrjabina A.S., Sohranskij V.B. Underground storage of helium // Izhevsk, IKI, 2015, p. 272. (in Russ.).
12. Bondarev V.L., Chugunov A.V., Sarkisova M.A.,. Bondarev Ye.V Outlooks for storing of heliumenriched natural gas in the Eastern Siberia and at the Far East // Moscow. Vesti gazovoy nauki 2015 №3(23), pp. 63-67. (in Russ.).
13. Malbrunot, P., Vidal, D., Vermesse, J., Chahine, R., Bose, T.K. Adsorbent Helium Density Measurement and Its Effect on Adsorption Isotherms at High Pressure // Langmuir, 13 (3), 1997, pp. 539-544.
14. Saha, D., Bao, Z., Jia, F., Deng, S. Adsorption of CO2, CH4, N2O, and N2 on MOF-5, MOF-177, and zeolite 5A. // Environ Science Technology, 2010, 44(5) pp.1820-1826.
15. Cavenati, S., Grande, C.A. and Rodrigues, A.E Adsorption Equilibrium of Methane, Carbon Dioxide, and Nitrogen on Zeolite 13X at High Pressures // Journal of Chemical & Engineering Data, 49 (4), 2004, pp. 1095–1101.
16. Maggs, F.A., Schwabe, P.H. and Williams, J.H. Adsorption of Helium on Carbons: Influence on Measurement of Density. // Nature, Volume 186, Issue 4729, 1960, pp. 956-958.
17. Sirotin S.A. Technology extraction of helium concentrate. Suggestions for helium purification technology. // Scientific and Technical Council OJSC «Gazprom», Orenburg, 7-8th September 2010 г. (in Russ.).
18. Das, N.K., Chaudhuri, H., Bhandari, R.K., Ghosh, D., Sen, P., Sinha, B. Purification of Helium from Natural Gas by Pressure Swing Adsorption. // Current Science. 95 (12), 2008, p. 1684-1691.
19. Dytnerskij Ju.I., Brykov. V.P., Kagramanov G.G. Membrane separation of gases. // Moscow, Himija, 1991, p. 344. (in Russ.).
20. Nikolaev N.I. Diffusion in membranes. // Moscow, Himija, 1980, p. 232. (in Russ.).
21. Noble R.D., Stern S.A.. Membrane Separations Technology - Principles and Applications. // Amsterdam, Elsevier, 1995, p. 738.
22. Baker R.W. Membrane technology and applications. Second edition. //. New York, John Wiley&Sons, 2004, p. 552.
23. Van Der Burg E., Miyagishima N., Itami Y. Spiral wound gas separation membrane module. WIPO Patent Application WO/2015/049499, 2015.
24. Gyu Hong Min, Fufang Zha. Hollow Fiber membrane module. U.S. Patent Application 20140183123, 2014
25. Takashi Monzen, Takahito Hirashima. Hollow-fiber membrane module. U.S. Patent 6623637, 2003.
26. Yoji Kase, Toshimune Yoshinaga, Kenji Fukunaga, Harutoshi Hoshino. Asymmetric hollow-fiber gas separation membrane, gas separation method and gas separation membrane module. U.S. Patent 7803214, 2010.
27. Хванг С.Т., Каммермейер К. Мембранные процессы разделения. Пер. с англ. Е.П. Моргуновой и Ю.И. Дытнерского // М.: Химия, 1981 C. 464. (in Russ.).
28. Nicholas P. Wynn. Gas separation membrane module assembly with residue manifold. U.S. Patent 7918921, 2011.
29. Nicholas P. Wynn, Donald A. Fulton. Gas separation membrane module assembly. U.S. Patent 7510594, 2009.

**Comparison of energy consumption of two types of freeze-drying in the preparation of materials with high porosity**

**Alexander Alexeyevich Didenko**, Ph. D.

Head of lyophilization department

NPO Petrovax Pharm, limited liability company

Zagorevskaya str., 10/4, Moscow, 115598

E\_mail: DidenkoAA@petrovax.ru

**Timofey Nikolaevich Somov**

Ph. D. Student, MUCTR, Geroev Panfilovchev, 20, Moscow, 125480

E\_mail: timofeysomov@gmail.commailto:DidenkoAA@petrovax.ru

**Natalia Vasilevna Menshutina**, Prof.

Director of International Science and Education Center for Transfer of Biopharmaceutical Technologies, MUCTR, Geroev Panfilovchev, 20, Moscow, 125480

E\_mail: chemcom@muctr.ru

Tel.: +74954950029

***Keywords:*** *vacuum freeze-drying, atmospheric freeze-drying, energy, porosity.*

In the course of this work it was investigated the effect of two methods of freeze drying on the porosity of the material, which was carried out in a vacuum freeze dryer (VFD) and atmospheric freeze dryer (AFD). Both processes differ in mobility of the material within the dryer and the method for supplying energy to the material. VFD is a classic drying trays, where the material in the drying process is stationary. AFD is operated at atmospheric pressure, where the material flow of cold air is dried while in a fluidized bed. The materials used were mannitol and dextran. For both methods of drying the energy costs of the process es were calculated and compared.

**Reference**

1. J. Jeff Schwegman Basic Cycle Development Techniques for Lyophilized Products // SP Scientific, 2009.
2. G.V. Semenov Vacuum freeze-drying. // M.: Deli Plus (Deli Plus), 2013.
3. Yu. D. Tretyakov, N. N. Oleinikov, O .A. Shlyakhtin Сryochemical Technology of Advanced Materials // London: Chapman&Hall, 1997.
4. P.N. Ezhilarasia, D. Indranib, B.S. Jenac, C. Anandharamakrishnana Freeze drying technique for microencapsulation of Garcinia fruit extract and its effect on bread quality// Journal of Food Engineering. V 117, I 4, 2013, P 513–520.
5. M. Mumenthaler, H. Leuenberger Atmospheric spray-freeze drying: a suitable alternative in freeze-drying technology // International Journal of Pharmaceutics. V 72, I 2, 1991, P 97–110.