**Mechanisms of activation in technology of zinc sulfides silicate and materials on their basis**

**Yusupova Alsu Ansarovna**

Ph.D of the Department of Technology of Inorganic Substances and Materials.

Kazan National Research Technological University

Address: 420088, Kazan, ul.Sibirski trakt, 12.

E-mail: [alsu16rus@yandex.ru](mailto:alsu16rus@yandex.ru)

**Sahabova Guzel Igorevna**

Ph.D of the Department of Technology of Inorganic Substances and Materials.

Kazan National Research Technological University

Address: 420097, Kazan, ul.Sibirski trakt, 12.

E-mail: guzja1987@mail.ru,

**Khatsrinov Aleksey Ilich**

Head of the Department of Technology of Inorganic Substances and Materials. Professor.

Kazan National Research Technological University

Address: 420097 Kazan, ul.Sibirski trakt, 12.

E-mail: khatsrin@mail.ru

**Ahmetova Rezida Timerhanovna**

Professor of the Department of Technology of Inorganic Substances and Materials

Kazan National Research Technological University

Professor of the Department of Technology of Inorganic Substances and Materials. Kazan National Research Technological University.

Address: 420012 Кazan, ul.Sibirski trakt, 12.

E-mail: rachel13@list.ru,

***Keywords****: sulfur activation mechanisms, zinc chloride, zinc silicate sulphide, quantum chemical calculations.*

A method has been developed for synthesizing inorganic zinc silicate sulphide, which consists in activation of the opening of the sulfuric ring by zinc chloride, which reduces the activation energy of the process, and at the same time, facilitates the chemical interaction of sulfur with surface silicon silicate. A comparative evaluation of the mechanisms of the disclosure of Cycloser molecules in the presence of zinc chloride and in its absence is given. The thermodynamic characteristics of various mechanisms of the attachment of diatomic sulfur to the surface of silicate have been calculated. The addition of sulfur to the atom of zinc fixed on the surface of silicate occurs with the lowest energy consumption. Developed on the basis of inorganic sulphide zinc silicate, sulfur materials have high physical-mechanical and operational properties. Optimal conditions of the synthesis process are determined.

**References**

1. Ismagilov F.R. Ways of ecological optimization of sulfur production at gas and oil refineries. Sera i sernay kislota - 2017: Sb. materialov 7-oy megdunarodnoy naychno-prakticheskoy konferensu [Sera and sulfuric acid - 2017: Sat. materials of the 7th International Scientific and Practical Conference], 2017, no. 7, pp. 28-31. (in Russ.).

2. Groshin A.P., Korolev E.V., Kalinkin E.G. Structure and properties of modified sulfur binder // Building materials. 2005. № 7. pp. 6-9.

3. Rau VG, Skvortsov KV, Potekhin K.A., Maleev A.V. Geometric analysis of molecular nanoclusters of sulfur (S8) x in a computer experiment // Journal of Structural Chemistry. 2011. № 4. T.52. C.781-786.

4. Reactions of sulfur with organic compounds / Ed. VN Voronkov. Novosibirsk. The science. 1979.

5. Lisichkin, G.V. Modified silica in sorption, catalysis and chromatography. // Moscow: Nauka, 1986.

6. VI Lygin. Models of "hard" and "soft" surfaces. The construction of the microstructure of the surface of silica // Ros. chem. f. (Zh.M., D. of the Chemical Society named after DI Mendeleyev). 2002. T. XLVI. № 3. P. 12-18

7. Aleskovsky V.B. Quantum synthesis // Zhurn. prikl. chemistry. 2007. -T. 80.- No. 11.- С. 1761-1767

8. Sabakhova GI, Akhmetova PT, Baraeva LR, Tuktarova AI, Lin AI, Akhmetova A. Yu. Influence of zinc chloride on the cross-linking ability of sulfur in the synthesis of zinc silicate sulphide // Vestnik Kazan Technological University .- 2013.- № 21.- P. 54-57.

**The use of a polymeric modifier to improve the quality of gypsum binder**

**Kostromina Natalya Vasiljevna**, Cand. Sci. (Tech.), Associate Professor of the Chair of plastics processing technology, D. Mendeleev University of Chemical Technology of Russia. Address: Miusskaya sq., 9, 125047 Moscow, Russia, 9, tel.: 8 (499) 978-97-96, e-mail: nkostromina@muctr.ru

**Osipchik Vladimir Semjenovich**, Dr. Sci. (Tech.), professor, professor of the Chair of plastics processing technology, D. Mendeleev University of Chemical Technology of Russia. Address: Miusskaya sq., 9, 125047 Moscow, Russia, 9, tel.: 8 (499) 978-80-20, e-mail: vosip@muсtr.ru

**Ivashkina Vera Nikolaevna**, Engineer of the Chair of plastics processing technology, D. Mendeleev University of Chemical Technology of Russia. Address: Miusskaya sq., 9, 125047 Moscow, Russia, 9, tel.: 8 (499) 978-97-96, e-mail: ivashkina@muctr.ru

**Aristov Vitalyj Mikhailovich**, Dr. Sci. (Physic.-mathemat.), professor, Chief of the Chair of plastics processing technology, D. Mendeleev University of Chemical Technology of Russia. Address: Miusskaya sq., 9, 125047 Moscow, Russia, 9, tel.: 8 (499) 978-82-64, e-mail: [aristov@muctr.ru](mailto:aristov@muctr.ru)

**Kozlovskiy Ivan Anatolievich**

Mendeleyev University of Chemical Technology of Russia,

Ph.D. in Chemistry. Chair of Technology of Base Organic and Petrochemical Synthesis. 125047, Moscow, Miusskaya sq. 9. Phone: +74999789288

***Keywords:*** *gypsum binders, organosilicon modifier, water consumption, physical and mechanical properties.*

In the article rational ways of improvement and increase of technological and operational properties of building gypsum are considered. Increase the strength, change the setting and hardening of gypsum by introducing modifying additives. The article deals with the application of composite gypsum binders, to improve the structure and properties of which the capabilities of the organosilicon modifier are used. The use of a silicon-organic modifier opens up wider possibilities in regulating the setting process of binders and creating optimal conditions for the formation of products. The technical result is the possibility of obtaining building materials with predictable properties in a wide range that improve the consumer properties of gypsum binders.

**References**

1. Korovyakov V.F., Burianov A.F. Scientific and technical prerequisites for the effective use of gypsum materials in construction. Zhilishnoe stroitelstvo [Housing construction], 2015, no. 12, рр. 38-40 (in Russ.).

2. Rozenkova I.V., Rumyantsev A.V. Hydrophobizers «NEOGARD» for building materials and structures. Stroitelnye materialy [Construction Materials], 2009, no. 6, рр. 20-21 (in Russ.).

3. Drebezgova M.Yu. The peculiarities of hydration of the composite gypsum binder in the presence of a superplasticizer SIKAPLAST 2135. Vestnik Belgorodskogo gosudarstvenogo tehnologicheskogo universiteta im. V.G.Shuhova [Bulletin of Belgorod state technological V. G. Shuhov University], 2017, no. 5, рр. 20-23 (in Russ.).

4. Brueckner H. Gypsum. Manufacture and use of gypsum building materials (translated from German). M.: Stroizdat, 1981. 223 p. (in Russ.).

5. Thole V. Strength and adhesion properties of polymer modified gypsum. ZKG: Zement - Kalk - Gips International [CLG: Cement - Lime - Gypsum International], 1999, no 7., рр. 400-406 (in Germany).

**Efficiency of reusing of pyroxyline gunpowders as the component of industrial explosives**

**Mikheev Denis Igolevich**

D.I. Mendeleev University of Chemical Technology of Russia, Senior lecturer of Technosphere Safety Department

Address: 125047, Moscow, Miusskaya Sq., 9;

e-mail: [mikheev@muctr.ru](mailto:mikheev@muctr.ru)

**Akinin Nikolay Ivanovich**

D.I. Mendeleev University of Chemical Technology of Russia, Head of Technosphere Safety Department, Doctor of Technical Sciences

Address: 125047, Moscow, Miusskaya Sq., 9;

Phone: +7 (495) 490-82-58

e-mail: [akinin@muctr.ru](mailto:akinin@muctr.ru)

**Annikov Vladimir Eduardovich**

D.I. Mendeleev University of Chemical Technology of Russia, Leading researcher, Candidate of Technical Sciences.

Address: 125047, Moscow, Miusskaya Sq., 9.

Тел. раб. +7 (495) 496-69-73;

e-mail: [veannikov@mail.ru](mailto:veannikov@mail.ru)

***Keyword:*** *ammunition utilization, single base propellants, industrial explosives, slurry explosives.*

The article considers the possibility of using single base propellants, including recovered from ammunition disposal, as energy-intensive components of slurry explosive compositions for industrial use. The results of experimental studies of detonation characteristics and safety parameters of those explosive compositions in comparison with TNT and standard industrial explosives are presented. The efficiency of drilling and blasting operations by gunpowder water-gel compositions was compared with the standard industrial explosive composition Ammonite №6ZhV. Based on the conducted studies, conclusion about the potential of the use of gunpowder water-gel compositions for drilling and blasting operations was made.

**References**

1. In the Armed Forces of the Russian Federation obsolete ammunition disposing by blasting method had ended, Russian Ministry of Defense website. Available at: https://function.mil.ru/news\_page/country/more.htm?id=11543183@egNews (Accessed at 01.03.2018,( in Russ.);

2. B.V. Maceevich, V.P. Glinskij, V.P. Vinnikov The role of industry in the process of disposing of conventional types of munitions, Aktual'nye problemy utilizacii raket i boepripasov. Sbornik dokladov [Actual problems of utilization of missiles and ammunition. Collection of reports], Moscow, Geodeziya, 2012, pp. 44-57. (in Russ.);

3. Collection of reports of Experience in the use of pyroxylin powders in engineering work, Kiev: Izdatel'stvo AN USSR, 1952, 112 pp. (in Russ.);

4. Frantov A.E. Conversion explosives - conditions of rational use in geotechnologies, LAP Lambert Academic Publishing, German, 2014. – 136 pp.;

5. Maceevich B.V., Shhukin Ju.G., Kolominov I.A., Chernyshov S.N., Lugov M.S., Fedoseev V.V Improvement of industrial explosives by using high-energy materials of recycled ammunition, Vzryvnoe delo [Explosion technology]. Vol. 117/75., M.: IPKON RAN, 2017, pp. 157-164 (in Russ.);

6. Actual problems of industrial utilization of missiles and ammunition. Safety, resource-saving, ecology. Collection of reports. – 2015. – 232 pp.; (in Russ.)

7. Andrzej Maranda, Katarzyna Lipiсska and Marek Lipiсski Demilitarized propellants as ingredients in commercial explosives, Brighton Conference Proceedings, 2005, pp. 493-498;

8. Peng Wang, Xiaoan Xei and Weidong He Preparation and Performance of a Novel Water Gel Explosive Containing Expired Propellant Grains, Central European Journal of Energetic Materials, 2013, Vol. 10(4), pp. 495-507;

9. Zajcev V.M., Pohil P.F., Shvedov K.K., Electromagnetic method for measuring the velocity of explosion products, Doklady AN SSSR [Reports of the USSR Academy of Sciences], 1960, vol. 132(6), pp. 1339-1340 (in Russ.);

10. Technical Regulations of Eurasian Customs Union "Safety of explosives and products on its base" (TR TS 028/2012), 23 pp. (in Russ.);

11. Shhukin Ju.G. Industrial explosives based on utilizing ammunition: Textbook for universities, Moscow, Nedra, 1998, 319 pp. (in Russ.);

12. Dremin A.N., Savrov S.D., Trofimov V.S., Shvedov K.K. Detonation waves in condensed media, M.:Izdatel'stvo «Nauka», 1970, -164 pp. (in Russ.);

13. GOST 21984-76 Industrial explosives. Ammonite N 6ZhV and ammonal waterproof. Technical specifications (in Russ.);

14. Nosyko F.L., Beljaev A.G., Doduh V.G. Emulsion explosive "Nitronit"®, Gornaja Promyshlennost' [Mining Industry] vol. 5 (111), 2013, pp. 24-26 (in Russ.);

15. GOST 4117-78 TNT for industrial explosives. Technical specifications (in Russ.);

16. Andreev K.K., Beljaev A.F. Theory of explosives, M.: nauchno tehnicheskoe izdatel'stvo OBORONGIZ, 1960, -596 p. (in Russ.);

17. Andreev K.K. Thermal decomposition and burning of explosives, M.: Izdatel'stvo «Nauka», 1966. ¬ 347 pp. (in Russ.);

18. Peng Wang, Xiaoan Xei, Weidong He Thermal Stability and Underwater Energy of Water Gel Explosive Using Expired Single-Base Propellants as Ingredients, Journal of Energetic Materials, Vol. 32, 2014, pp. 51–59;

19. Bulycheva T.I., Miheev D.I., Akinin N.I., Trunin V.V. Decrease of ecotoxicity of gunpowder water-gel compositions, Sb. Materialov II mezhdunarodnoj nauchno-prakticheskoj konferencii molodyh uchenyh po problemam tehnosfernoj bezopasnosti [The II International Scientific and Practical Conference of Young Scientists on Problems of Technosphere Safety. Collection of Reports], M.: Izdatel'skij centr RHTU im. Mendeleeva, 2017, pp. 52-54 (in Russ.);

20. Doroshenko S.I., Mihajlov N.P. and others, Efficiency of gunpowder explosives application on gel basis in engineering, Pjataja mezhdunarodnaja nauchnaja konferencija Fizicheskie problemy razrushenija gornyh porod. Zapiski Gornogo institute [The Fifth International Scientific Conference "Physical Problems of Rock Destruction". Notes of the Mining Institute], Vol.171, 2007. – S-Pb.: SPGGI (TU), pp. 150-152 (in Russ.);

21. Annikov V.E., Akinin N.I., Mikheev D.I., Soboleva L.I., Derzhavets A.S., Brigadin I.V., Doroshenko S.I. About features of detonation and impact on rock by powder water gel explosives, Gorny informatsionno-analiticheskiy byulleten [Mining informational and analytical bulletin], Moscow, 2015, vol. 12, pp. 318 – 324 (in Russ.);

22. Semenjak S.Ju. Use of a gelpore for blasting mining in quarries for the production of building material, Gorny informatsionno-analiticheskiy byulleten [Mining informational and analytical bulletin], Moscow, 2005, Vol. 8. - pp. 172– 174 (in Russ.).

**Design of high pressure apparatus for supercritical processes**

**Menshutina Natalya V.**

Dmitry Mendeleev University of Chemical Technology of Russia, Head of Russian-Swiss science and education center for Transfer of biopharmaceutical technologies, D. Sc. (engineering), professor. Moscow, Geroev Panfilovtsev st. 20

E-mail: [chemcom@muctr.ru](mailto:chemcom@muctr.ru). Tel.:+74954950029

**Tsygankov Pavel Yu.**

Dmitry Mendeleev University of Chemical Technology of Russia, Russian-Swiss science and education center for Transfer of biopharmaceutical technologies, p.h.d. student. Moscow, Geroev Panfilovtsev st. 20. E-mail: [pavel.yur.tsygankov@gmail.com](mailto:pavel.yur.tsygankov@gmail.com). Tel.:+74954950029

**Lebedev Evgeniy A.**

Dmitry Mendeleev University of Chemical Technology of Russia, Russian-Swiss science and education center for Transfer of biopharmaceutical technologies, p.h.d.

Moscow, Geroev Panfilovtsev st. 20. E-mail: [e.a.lebedev@gmail.com](mailto:e.a.lebedev@gmail.com).

Tel.:+74954950029

**Lebedev Artem E.**

Dmitry Mendeleev University of Chemical Technology of Russia, Russian-Swiss science and education center for Transfer of biopharmaceutical technologies, p.h.d.

Moscow, Geroev Panfilovtsev st. 20. E-mail: [artem.evg.lebedev@gmail.com](mailto:artem.evg.lebedev@gmail.com).

Tel.:+74954950029

***Keywords:*** *supercritical fluid, supercritical process, high pressure apparatus.*

Conducting processes under supercritical conditions requires appropriate high-pressure apparatus. This paper is focused on development stages of high pressure apparatus for supercritical processes. High-pressure apparatus' working part design was developed on the basis of the results of supercritical carbon dioxide hydrodynamics mathematical modeling. To do this, modern computer simulation methods, based on principles of computational fluid dynamics (CFD), were used. Detailed engineering and strength calculations were carried out for the developed basic design. The designed apparatus was manufactured and successfully commissioned.

**References**

1. Noyori R. Pursuing practical elegance in chemical synthesis // Chemical Communications. ‒ 2005. № 14. ‒ pp. 1807-1811.

2. Cornelio-Santiago H. P., Gonçalves C. B., de Oliveira N. A., de Oliveira A. L. Supercritical CO 2 extraction of oil from green coffee beans: solubility, triacylglycerol composition, thermophysical properties and thermodynamic modelling // The Journal of Supercritical Fluids. ‒ 2017.

3. da Silva R. P., Rocha-Santos T. A., Duarte A. C. Supercritical fluid extraction of bioactive compounds // TrAC Trends in Analytical Chemistry. ‒ 2016. ‒ Vol. 76. ‒ pp. 40-51.

4. Desfontaine V., Guillarme D., Francotte E., Nováková L. Supercritical fluid chromatography in pharmaceutical analysis // Journal of pharmaceutical and biomedical analysis. ‒ 2015. ‒ Vol. 113. ‒ pp. 56-71.

5. Płotka J. M., Biziuk M., Morrison C., Namieśnik J. Pharmaceutical and forensic drug applications of chiral supercritical fluid chromatography // TrAC Trends in Analytical Chemistry. ‒ 2014. ‒ Vol. 56. ‒ pp. 74-89.

6. Gorle B., Smirnova I., Arlt W. Adsorptive crystallization of benzoic acid in aerogels from supercritical solutions // The Journal of Supercritical Fluids. ‒ 2010. ‒ Vol. 52, № 3. ‒ pp. 249-257.

7. Smirnova I., Mamic J., Arlt W. Adsorption of drugs on silica aerogels // Langmuir. ‒ 2003. ‒ Vol. 19, № 20. ‒ pp. 8521-8525.

8. Bahrami M., Ranjbarian S. Production of micro-and nano-composite particles by supercritical carbon dioxide // The Journal of Supercritical Fluids. ‒ 2007. ‒ Vol. 40, № 2. ‒ pp. 263-283.

9. Eckert C. A., Knutson B. L., Debenedetti P. G. Supercritical fluids as solvents for chemical and materials processing // Nature. ‒ 1996. ‒ Vol. 383, № 6598. ‒ pp. 313.

10. Dillow A. K., Langer R. S., Foster N., Hrkach J. S. Supercritical fluid sterilization method // Book Supercritical fluid sterilization method / EditorGoogle Patents, 2000.

11. Zhang J., Davis T. A., Matthews M. A., Drews M. J., LaBerge M., An Y. H. Sterilization using high-pressure carbon dioxide // The Journal of Supercritical Fluids. ‒ 2006. ‒ Vol. 38, № 3. ‒ pp. 354-372.

12. Perrut M. Sterilization and virus inactivation by supercritical fluids (a review) // The Journal of Supercritical Fluids. ‒ 2012. ‒ Vol. 66. ‒ pp. 359-371.

**Heavy metals containing wastewater purification by nanofiltration and ion exchange methods**

**Lin Maung Maung**., post graduated student, Mendeleev University of Chemical Technology of Russia, Department of Membrane Technology, Moscow, Russia Federation; e-mail: e-mail: linmg51@gmail.com

**Farnosova Elena** N., Ph.D. (tech.), docent Mendeleev University of Chemical Technology of Russia, Department of Membrane Technology, Moscow, Russia Federation; e-mail: e-mail: farelena@rambler.ru

**Kagramanov Georgiy** G., Doctor of science (tech.), chef of the chair, Mendeleev University of Chemical Technology of Russia, Department of Membrane Technology, Moscow, Russia Federation, tel. +7(499) 978-82-60; e-mail: kadri@muctr.ru

***Keywords:*** *membrane separation, nanofiltration, ion exchange, exchange capacity, heavy metals.*

Many useful and effective methods of wastewater treatment and water purification technologies are chemical, physicochemical, electrochemical and etc. The technologies of nanofiltration and ion exchange are widely used for the purification of wastewater, containing heavy metals, to decrease the environmental and ecological risks. Nanofiltration and ion exchange characteristics of wastewater purification from heavy metals have been studied. The influence of basic process parameters – temperature, pressure, concentration and pH value of the feed solution on flux and rejection of nanofiltration membranes has been considered. The ion exchange capacities of resins in the removal of heavy metal ions from wastewater have been determined.

**References**

1. P.S. Sudilovski., G.G. Kagramanov., V.A. Kolesnikov. Use of RO and NF for treatment of copper containing wastewaters in combination with flotation // Desalination, 2008, vol. 221, pp 192 – 201.

2. Department of membrane technology, Terminology [electronic resource]. Access: http://www.membrane.msk.ru/term/ (date treatment 15.10.15) ( in Russ).

3. H.K. Shon., S. Phuntsho., D.S. Chaudhary., S. Vigneswaran., J. Cho. Nanofiltration for water and wastewater treatment – a mini review // Drinking Water Engineering Science – Discuss, 2013, vol. 6, pp 47 – 53.

4. D.W. Sundstrom., H.E. Klei. Wastewater Treatment // Department of Chemical Engineering, The University of Connecticut by Prentice-Hall, Inc., Englewood Cliffs, N.J. 07632, pp 356.

5. Nurasyikin Misdan., Woei Jye Lau., Chi Siang Ong., Ahmad Fauzi Ismail., Takeshi Matsuura. Study on the thin film composite poly (piperazine-amide) nanofiltration membranes made of different polymeric substrates: Effect of operating conditions // Korean Journal of Chemical Engineering, 2015, vol. 32, pp 753 – 760.

6. J.J. Qin., M.H. Oo., H. Lee., B. Coniglio. Effect of feed pH on permeate pH and ion rejection under acidic conditions in NF process // Journal of Membrane Science, 2004, vol. 232, pp 153 – 159.

7. J. Tanninen., M. Nystrom. Separation of ions in acidic conditions using NF // Desalination, 2002, vol. 147, pp 295 – 299.

8. J.J. Qin., M.H. Oo., M.N. Wai., F.S. Wong. Effect of feed pH on an integrated membrane process for the reclamation of a combined rinse water from electroless nickel-plating; Journal of Membrane Science, 2003, vol. 217, pp 261 – 268.

9. J.M.M. Peeters., M.H.V. Mulder., H. Strathmann. Streaming potential measurements as a characterization method for nanofiltration membranes // Colloids and Surfaces A: Physicochemical and Engineering Aspects, 1999, vol. 150, pp 247 – 259.

10. J.J. Qin., M.N. Wai., M.H. Oo., F.S. Wong. A feasibility study on the treatment and recycling of a wastewater from metal plating // Journal of Membrane Science, 2002, vol. 208, pp 213 – 222.

11. N.V. Golovaneva., G.G. Kagramanov., Ye.N. Farnosova. Nanofiltration water purging of hardness salts // Water: Chemistry and Ecology, 2014, №5, pp 36 – 41 (in Russ.).

12. B.A.M Al-Rashdi., D.J. Johnson., N. Hilal. Removal of heavy metal ions by nanofiltration // Desalination, 2013, vol.315, pp 2 – 17.

13. J. Schaep., B. Van der Bruggen., C. Vandecasteele., D. Wilms. Retention Mechanisms in Nanofiltration // Chemistry for the protection of the environment 3, 1998, Vol.55, pp 117 – 125.

14. A. Dabrowski., Z. Hubicki., P. Podkoscielny., E. Robens. Selective removal of the heavy metal ions from waters and industrial wastewaters by ion exchange method // Chemosphere, 2004, vol. 56, pp 91 – 106.

**The use of coagulants based on titanium and silicon chlorides in the purification of the filtrate of the solid municipal waste landfill**

**Krutchinina Nataiya,** Dr. Sci. professor, Head of the Faculty of Biotechnology and Industrial Ecology, Head of the department of Industrial Ecology e-mail: [krutch@muctr.ru](mailto:krutch@muctr.ru)

**Kuzin Evgeniy**, Chief of laboratory of Industrial Ecology, e-mail: [e.n.kuzin@mail.ru](mailto:e.n.kuzin@mail.ru)

**AzopkovSergey**, First rank engineer, e-mail: [sergej.azopkov@mail.ru](mailto:sergej.azopkov@mail.ru)

Dean, Dmitry Mendeleev University of Chemical Technology of Russia, 125047 Russia, Moscow, Miusskaya Square 9

***Keywords****: filtrate of TKO polygon, coagulation, titanium and silicon chlorides.*

The issue of cleaning the filtrate of solid municipal waste landfills is a complex and urgent task. Today, the most effective technology for the purification of filtrate is membrane systems, but for their successful operation, the wastewater must undergo a pre-treatment stage. A promising direction of reagent processing is the use of titanium and silicon compounds as coagulants. In the course of the work, an assessment was made of the possibility of using coagulants based those elements compounds in the purification processes of the filtrate of solid municipal waste landfills. It has been established that titanium chlorides are significantly superior in purification efficiency to the most common coagulants (aluminum sulphate and ferric chloride).

**References**

1. ТBN 30-308-2002 "Designing, construction and reclamation of landfills of solid household waste in the Moscow Region" ( in Russ ).

2. Glushankova I.S. Avtoreferat dissertacii d.t.n. Purification of filtration waters of landfills of burial of solid household waste at various stages of the life cycle Author's abstract of the dissertation - Perm' – 2004 - 52 p. ( in Russ ).

3. Draginskij V. L., Alekseeva L. P., Getmancev S. V. Coagulation in the technology of natural water purification. M., Nauch. izd. 2005. 576 p. ( in Russ ).

4. Ostrovkin I. M., Ostrovkin P. I. Method for cleaning the leachate of the landfill for solid domestic waste Patent № 2400437 RU. № 2009135301/05, publ. 10.09.2012 ( in Russ ).

5. Gonopol'skij A. M., Martynov P. N., Mitashova N. I., Nikolajkina N. E., Podzorova E. A., CHaban' A. YU. Method for cleaning the leachate of the landfill for solid domestic waste Patent № 2401250 RU. № 2009134291/05 . publ. 10.10.2010( in Russ ).

6. Frog B. N., Levchenko A. P. Water treatment: Inst. manual for universities. Moscow: MSU Publishing House , 1996. 680 p( in Russ ).

7. GOST R 52769-2007 Methods for determining chroma( in Russ ).

8. ERD F Ф 14.1; 2.110-97 Method for performing measurements of the contents of suspended solids and total impurities in samples of natural and treated wastewater ( in Russ ).

9. GOST R 55684-2013 Method for determination of permanganate oxidizability ( in Russ ).

10. Luchinskij G.P. Chemistry of titanium М .: Publishing house "Himiya" [Chemistry] , 1971. – 471 p. (in Russ ).

11. SHabanova N.A., Popov V.V., Sarkisov P.D. Chemistry and technology of nanodispersed oxides. Tutorial. Moscow: Academic Library,IKC «Akademkniga», 2007. 309 p. ( in Russ ).

12. Maslennikov A. N. Preparation of titanium tetrachloride from the titanium raw material of the Yaregsky deposit by fluidized bed chlorination :dis. Author's abstract of the dissertation. - Moscow. -2018 - 18 p. ( in Russ).

13. Evstratova K.I. Physical and colloid chemistry. M .: Publisher: Vysshaya shkola [High school] , 1990, 487 p. ( in Russ ).

14. N.E. Krutchinina, E. N, Kuzin, S.V. Azopkov, I.A. CHechikov, D.YU. Petruhin Modification of titanium coagulant by sulphate method // Ecology and industry Moscow , 2017. № 2.–S.P. 24-27 (in Russ).

15. Izmajlova N. L. Coagulation and heterocoagulation processes in the water system microcrystalline cellulose - titanium dioxide - titanyl sulfate: dissertation Sankt-Peterburg. 2013. 189 p. ( in Russ ).

16. Gonopol'skij A.M., Nikolajkina N.E., Murashov V.E., Mitashova N.I., Kushnir K.YA. Multistage technology for cleaning the filtrate of landfills of solid domestic waste // Water: chemistry and ecology — 2008. — № 2. — P. 25-30. (in Russ).

17. Gonopol'skij A.M., Stompel' S.I., Ladygin K.V. A rhetorical generalization of the results of experimental studies of the ultrasonic purification process of reverse osmosis membranes. Ecology and industry of Russia, No8, 2014, P. 28 -31 (in Russ).

**The development of computer models of industrial technological scheme of the process thermo-oxidative destruction of the sludge**

**Sovetin Filipp Sergeevich,** PHD, associate professor of the Department of Informatics & computer design of the D. Mendeleev University.

e-mail: [fsovetin@inbox.lv](mailto:fsovetin@inbox.lv) и [fsovetin@rambler.ru](mailto:fsovetin@rambler.ru)

Phone: +7(499)-978-84-18

**Shatalov Kirill Ilich**, doctor PHD, associate professor of the Departament of General & inorganic chemistry of the D. Mendeleev University.

e-mail: kirill\_shatalov@mail.ru

Phone: +7(499)-978-75-85

**Gartman Tamas Nikolaevich,** doctor Habilitation, director of the Department of Informatics & computer design of the D. Mendeleev University;

e-mail: [gartman@muctr.ru](mailto:gartman@muctr.ru)

Phone: +7 (499)-973-12-85, (499)-978-84-11;

**Aseev Kirill Mihailovich**, system administrator of the Department of Informatics & computer design of the D. Mendeleev University.

e-mail: vipertree@gmail.com

Phones: +7(499)-978-84-18.

**Shumakova Olga Petrovna**, doctor PHD, associate professor of the Department of Informatics & computer design of the D. Mendeleev University; e-mail: fix.shumakova@yandex.ru

Phone: +7(499)-978-84-18

**Klushin Dmitri Vitalievich**, doctor PHD, associate professor of the Department of Informatics & computer design of the D. Mendeleev University;

e-mail: dklushin@gmail.com

Phone: +7(499)-978-84-18

***Keywords:*** *Modeling, cracking, reactor, computer model, module.*

The computer model of the technological scheme of the process of oxidative destruction of the tar has been developed and realized. Is proposed to simulate the process of thermo-oxidative cracking in the reactor by using model components. Researched various options for technological design of the technological mode of the distillation of this production. Computer models of three different technological lines of distillation were created and realized. Is concluded that the technological scheme of distillation with the complex column have the lowest heat duty. The most energy-saving technological scheme of the distillation of the mixture of products of oxidative destruction of tar is chosen that is actual for resolve problems of the energy saving in the petrochemical industry.

**References**

1. Zolotukhin V. A. Deep processing of heavy oil and petroleum residues // Sfera Neftegaz. No. 4. 2012. C. 70-75. (in Russ.)

2. Vorobiev, Yu., Kuzmin A. P. Chemical processes in organic liquids initiated by hydrodynamic activator // Bulletin of Tambov state technical University. 2012. Volume 18. No. 4. C. 905-911. (in Russ.)

3. Hanigan, V. L., Litvintsev I. Yu., Shvets V. F., Moroz I. V., etc. Deep thermal cracking of heavy oil residues, initiated by the ozone //Chemical industry today. 2004. No. 12. S. 31-40. (in Russ.)

4. Galiev R. G., Luhansk A. I., Tretyakov V. F., Ivanov A. N. The initiation of the process of thermal cracking of heavy oil residues oxygen-air // World of petroleum products. Bulletin of oil companies. 2007. No. 8. C. 16-19. (in Russ.)

5. Galiev R. G., Luhansk A. I., Moroz I. V., Ermakov A. N. Study of the mechanism of activation of the thermal cracking of tar with oxygen in the air // World of petroleum products. Bulletin of oil companies. 2008. No. 7. C. 16-19. (in Russ.)

6. Suchkov Y. P., Kozlovsky R. A., Shvets V. F., A. V. Gorbunov, A. I. Luhansk Method of thermal-oxidative cracking of heavy oil residues // Butlerov communications. 2014. Vol. 37. No. 2. C. 60-65. (in Russ.)

7. Shvets V. F., Suchkov Yu. P., Kozlovsky R. A., Lugansky A. I.,

Gorbunov A.V. thermal-Oxidative cracking of black oil. The study process in a flow reactor // Chemical industry today. 2013. No. 10. C. 19-25. (in Russ.)

8. Shvets V. F., Makarov M. G., Luhansk A. I., Gorbunov A.V., Suchkov Y. P., Staroverov D. V., Digurov N. G. Mathematical model of the process of thermal cracking of tar oil // Chemical industry today. 2012. No. 7. C. 51-53. (in Russ.)

9. Ziyatdinov N.N. Computer simulation and optimization in chemical technology // Theoretical Foundations of Chemical Engineering. 2014. V. 48. № 5. P. 539-540.

10. Kulov N.N., Gordeev L.S. Mathematical modeling in chemical engineering and biotechnology // Theoretical Foundations of Chemical Engineering. 2014. V. 48. № 3. P. 225-230.

11. Shvets V.F., Sapunov V. N., Kozlovskii R. A., Makarov M. G., Gartman T. N., Luganskii A. I., Sovetin F. S., Suckov Y. P., Gorbunov A. V. New ways to increase the depth of crude oil refining // Russian Journal of Applied Chemistry. T. 89, № 11. P. 1806-1815.

12. Sometin F. C., Gordievsky, Y. I., Hartmann T. N., Novikov D. K. Analytical review of approaches to modeling of processes initiated by cracking // Chemical industry today. No. 1. 2017. C. 3-15. (in Russ.)

13. Luhansk A. I. fundamentals of the process initiated by cracking of tar. Diss. ….... kand. tech. sciences'. M. rkhtu im. D. I. Mendeleev. 2015. (in Russ.)

14. Shvets V. F., Sapunov V. N., Kozlovsky R. A., Makarov M. G., Gartman T. N.,

Luhansk A. I., Sowetan F. S., Suchkov Y. P., Gorbunov A. V. Some variants of deepening of oil processing // Journal of applied chemistry. Vol. 89, Vol. 11. 2016. C. 114-125. (in Russ.)

16. Gartman T. N., Sovetin F. S., Podsekina Yu. I., Shvets V. F., Kozlovskii R. A., Sapunov V. N. Kinetic Simulation of Initiated Cracking of Tar // Theoretical Foundations of Chemical Engineering, 2018, T. 52, №. 1, P. 57–63.

17. Gartman T. N., Sovetin F. S. Analytical review of the modern packages of simulation programs for computer modeling of chemical-technological systems // Successes in chemistry and chemical technology. 2012. Vol. 26. No. 11 (140). P. 117 to 120. (in Russ.)

**Innovative Development Concept of Perspective Plant Protection Means in the Russian Federation ©**

**Babkin Valeriy,** Doctor of chemical science, academician, corresponding member of Russian Engineering Academy, professor, IICPME president, bureau member of Russian State Duma Expert Council

**Promonenkov Victor** Kirillovich – d.c.s., professor, laureate of the Russian State Prize, Molecular Diagnostics Institute, IICPME vise-president

**Ovcharenko Mikhail** Mikhailovich – d.a.s., professor, National Agrochemical Union president, IICPME vise-president

**Lubimov Alexey** Pavlovich – j.s.d., academician, Head of Diplomatic Academy Intenational Law Center of Russian Foreign Ministry. International Institute for Applied Сhеmistry Problems of the Modern Economy (IICPME), 1 Golutvinskiy lane, Moscow 119180,   
tel.: +7 (495) 935-83-55; e-mail: info@iicpme.com

***Keywords****: variation synthesis, pesticide, plant protection product, PPP, matrix structure, new active substance, innovation, project.*

The article is conceptual. It is a way to introduce a new approach to plant protection products (PPP) in Russian Federation – Variation Synthesis of Natural Derived Matrix Structures©.

Concept implementation is able to unite efforts of scientists and specialists of Russian Academy of Sciences, Higher School and applied institutes to accelerate scientific search and industrial release of fundamentally new domestic active substances with higher efficiency, environmentally positive and accessible, to enforce sovereignty of economy. It provides a brief analysis of domestic PPP active substances production in Russia.

International Institute for Applied Сhеmistry Problems of the Modern Economy (IICPME)

**References**

1. Arefiev N.V., Mozjaev E.E. Alternative energy and "Soap bubble" economy. Representative Power - 21st century [Predstavitel’naya vlast’ – XXI vek], 2018, no. 3, pp. 23-27 (in Russ.).

2. Epifanova O.N., Mischenko V.A. Some legislative support issues for development of Far North regions and Arctic zone of Russian Federation. Representative Power - 21st century [Predstavitel’naya vlast’ – XXI vek], 2018, no. 1-2, pp. 21-24 (in Russ.).

3. Ivanova N.I. National innovation systems, 2002. р. 6 (in Russ.).

4. Karpikov P.A., Lubimova L.P. Topical marking issues in Russia (on the example of pharmaceutical business). Actual issues of economics, management and law: a collection of scientific papers (yearbook) [Actual’niye voprosi economiki, upravleniya i prava: sbornik nauchnikh trudov (ezjegodnik)]. 2017, no. 2-3, pp. 47-54 (in Russ.).

5. Kudriaviy V.V. Russian power industry in comparison with the Soviet and foreign experience. Representative Power - 21st century [Predstavitel’naya vlast’ – XXI vek], 2016, no. 7-8, pp. 41-50 (in Russ.).

6. Lubimov A.P. Prospects for Russian innovation clusters development. Representative Power - 21st century [Predstavitel’naya vlast’ – XXI vek], 2013, no. 5-6, pp. 14-19 (in Russ.).

7. Lubimov A.P. Russian National Concept of Innovation System development (part 1). Representative Power - 21st century [Predstavitel’naya vlast’ – XXI vek], 2011, no. 7-8, pp. 24-29 (in Russ.).

8. Lubimov A.P. Russian National Concept of Innovation System development (part 2). Representative Power - 21st century [Predstavitel’naya vlast’ – XXI vek], 2012, no. 2-3, pp. 9-14 (in Russ.).

9. Lubimov A.P. From information, information processes and technologies to nanotechnology. Interview with Nobel laureate, State Duma deputy, academician and vice-president of RAS J.I. Alferov. Representative Power - 21st century [Predstavitel’naya vlast’ – XXI vek], 2009, no. 4, pp. 1-5 (in Russ.).

10. Lubimov A.P. Review of the book by Marenkov N.L. "Methodology of future innovation market infrastructure in Russia", 2005. Representative Power - 21st century [Predstavitel’naya vlast’ – XXI vek], 2006, no. 5, pp. 34-35 (in Russ.).

11. Lubimov A.P. Advantages and shortcomings of two important draft laws: expert opinions. Roundtable in the State Duma. Russian Law Journal [Jurnal Rossiyskogo prava]. 2000, no. 4, pp. 26-27 (in Russ.).

12. Lubimov A.P. Andreeva T.V. "Green" bonds as a tool for sustainable development projects investment. Representative Power - 21st century [Predstavitel’naya vlast’ – XXI vek], 2018, no. 4, рр. 21-26 (in Russ.).

13. Malugin I.N. Innovations can help mankind to overcome hunger. Actual issues of economics, management and law: a collection of scientific papers (yearbook) [Actual’niye voprosi economiki, upravleniya i prava: sbornik nauchnikh trudov (ezjegodnik)]. 2015, no. 4, pp. 21-30 (in Russ.).

14. Chekmarev P.A., Mal’ko A.M., other authors, Minselkhoz Rossii. Crops Phytosanitary Conditions Overview in Russia for 2017, and prediction of the of harmful objects development for 2018. FGBU Rosselkhozcenter. 2018, p. 544

(in Russ.).

15. State Catalog of Pesticides and Agrochemicals Permitted for Use in the Territory of the Russian Federation by October 6, 2017. Part 1. Pesticides. Reference book. Agrorus. 2018 (in Russ.).